Please read carefully this file before installing the Meta Kernel


A 128 Kb RAM card (or 256 or 512) is needed to install the Meta Kernel. 

1-Unprotect the card if necessary and merge it with MERGE1 (in the Left shift-
Library menu). 

2-Empty the whole port 0. For instructions, read chapter 28 of the User's Guide.
If there is no important data in your calculator, it is easier to initialize
it by pressing simultaneously the keys ON, A and F, and
answering NO. 

3-Transfer the program named RECV.KER from the PC to the calculator,
with XMODEM or KERMIT.

4-Then transfer the file MDGDEMO.KER. XMODEM is recommended, because of the
huge size of this file. In order to use XMODEM, with an HP48 REV R, just use
the built-in command XRECV. With an HP48 REV M or P, first send the file
XRECV.PRG from the PC to the calculator, then use it as if it was the standard
XRECV command.

5-On the calculator, put the name of this file on the stack ('MDGDEMO.KER'),
and execute the program RECV.KER. 

6-After a short time, the Meta Kernel is installed.

If you have any problems, write to :
hydrix.mdgdemo@epita.fr
